Name:         Ignore Dialtone
Version:      1.0fc1
Released:     February 2, 1995
Description:  The enclosed patcher, Ignore Dialtone, enables blind dialing on LaserWriter 16/600 PS International PostScript Fax Modems, so the modem will dial without waiting for dialtone.

The enclosed file is a self-extracting archive. To use, download, double-click the downloaded file (this decompresses it).

Note that this only works with the LaserWriter 16/600 PS International modem, also known as the "WorldModem."

To use this patcher:
  1. Open the Chooser and select a LaserWriter 16/600 PS having an 
     International Fax Modem.  Close Chooser.

  2. Launch the Ignore Dialtone patcher.

Thereafter, your fax modem will not wait for a dialtone prior to dialing.  This change will be in effect until you power cycle your printer.