Name:         PC Setup DIMM Patch
Version:      n/a
Released:     August 20, 1996
Description:  Corrects the problem of not being able
              to use large DIMMs (32 or 64 MB) with
              the 12" PC Compatibility Card. Instructions
              for using the patch are below.

This software consists of a self-extracting archive. To use, download, double-click the downloaded file (this decompresses it). 

This archive contains files that will correct the problem of using large (32 or 64 MB) DIMMs with the 12" PC Compatibility Card. Instructions for using the patch are below. This archive contains two different fixes for the same problem. Either method can be used.

IMPORTANT NOTE:  Supported DIMMs must be 2K refresh, fast-page mode, and symmetrical.  Neither EDO nor asymmetrical DIMMs are supported.  The 12" PC Compatibility Card will also support 4K refresh DIMMs, but the 7" PC Compatibility Card will not.  Please consult your memory vendor for details regarding their DRAM specifications.

This fix can be installed on other PC/DOS Compatibility Cards but it will not do anything differently unless it is used with the 12" PC Compatibility Card.
-----

PC Setup 1.5 Large DIMM patch

This is a patch file that contains an update to the PC Setup BIOS for the 12" PC Compatible card.  This patch will only modify PC Setup 1.5.  Do not attempt to patch or use anything else!

After the patch is installed, select Shutdown from the Special menu.  Do not select Restart.
-----

PC "DIMM.SYS" driver

This is the same patch in the form of a DOS driver.  To use, copy "DIMM.SYS" to the C: drive and add this line, as the first line, to the CONFIG.SYS file:

DEVICE=C:\DIMM.SYS

After that, restart the PC.
