Name:         LaserWriter Fax Tune Up
Version:      1.0
Rereleased:   November 6, 1996
Description:
Utility to prevent problems when printing oversize faxes to
only Apple LaserWriter printers with a PostScript Fax card 
(LaserWriter Select 360f & LaserWriter Pro 810f).

Path to this software:
  Apple SW Updates
    US
      Macintosh
        Printing
          LaserWriter
            LW Fax Tuneup 1.0

This software consists of a self-extracting archive. To use,
download, double-click the downloaded file (this
decompresses it).

From the Fax Tune-Up Read Me:

Using LaserWriter Fax Tune-Up

WHY The fax tune-up program prevents certain problems when
you print out oversize faxes on your LaserWriter printer.

If you receive banner-size or legal-size faxes, your printer
will reduce the fax to fit the paper size that is in the
largest-size paper tray you have installed (letter, A4, or
legal).

If you receive letter-size faxes with no margins, your
printer will reduce the fax to fit letter-size paper with
margins.

HOW 1. Open the Chooser and make sure that the printer you
use for your faxes is selected. 2. Open the fax tune-up
program.

IMPORTANT If you have restarted your printer, or turned it
off and then on again, you have to open the fax tune-up
program AGAIN before using your printer to print out
oversize faxes. The printer keeps the instructions it
receives from the fax tune-up program in its memory, and it
loses those instructions when it is turned off or restarted.
