      
LaserWriter Pro 810 For Windows

Copyright 1994 Apple Computer, Inc.

The enclosed file is a self-extracting archive of a Disk Copy 720K DOS disk
image.  To use, download, double-click the downloaded file (this decompresses
it), and use Disk Copy to create a disk.

Disk Copy can be found in the Utilties folder posted here.

SOFTWARE FOR WINDOWS 3.1  Ver. 3.56.1.08  10/4/93

Windows is a registered trademark of Microsoft Corporation. This file contains late-breaking news about your LaserWriter Pro 810 printer  and printing with Windows 3.1.  Some of this information may not be included in your "User's Guide".  To print this file, double click on Notepad icon, open this file and print.

DISKETTE CONTENTS
=================
README.TXT         This file
APPLEPS.DRV        Driver file for Windows 3.1 
PSCRIPT.HLP        On-Line help file 
LWPRO810.WPD       Windows Printer Description file for LaserWriter Pro 810
LWPRO810.PPD       PostScript Printer Description file for LaserWriter Pro 810
OEMSETUP.INF       Windows Installation setup file for this driver
USER HINTS

If you have any difficulties during installation of this drivers, refer to Chapter 6 (Print Manager) in the Windows 3.1 User's Guide for information about installing printer drivers.

KNOWN LIMITATIONS
=================

1. Mixed orientation mode printing from the same bin has unpredictable results.

2. Mixed bin printing from two bins of the same size or different page orientations has unpredictable results.

3. When printing an EPS file in landscape mode the EPS file may image 180 degrees relative to the application's image. This can be corrected by editing the WIN.INI file.  (Note: before making any changes to your WIN.INI file make a backup copy first.)- Using the Notepad editor or any other text editor of your choice, open WIN.INI file which exists in your Windows directory.- Search for the name of whichever printer you have installed until you findthe line that states the printer name and the port it is assigned to (example:   [LaserWriter PRO 810, LPT1] ).- Add the statement "landscapeorient=270" to the [specific printer, port]section. Now insert "landscapeorient=270" below the last line of the group.- Add one blank line and save the WIN.INI file.

4. Corel Draw V2.0 will work with this driver successfully, only if you introduce the driver in CORELDRW.INI file in your Corel directory. Open CORELDRW.INI file using Notepad, or Write, and then under [coreldrivers] add a line:   APPLEPS=1

5. When using Manual Feed operation for A4 is SEF ( Short Edge Feed), and for Letter paper size is LEF ( long Edge Feed) only.

6. Although some paper sizes may not be available for some specific papersource selection (i.e.: A3 or Ledger for Multimedia Power Feeder, the complete list of paper sizes is displayed for all paper sources in Printer Setup.

7. When a new paper source is selected in the Printer Setup Dialog box, the selected paper size switches to the default selection ( Letter).

8. B5 paper size can be used only with the Cassette or Manual feed.

9. Applications with Printer Setup for paper size as seen in MS-Write, Paintbrush, Notepad, and CorelDraw! v3.0 will not have SEF LETTER or A4 paper size available.